# (C) Copyright 2005- ECMWF.

unsigned[4] Ni : can_be_missing,dump;
alias numberOfPointsAlongAParallel=Ni;
alias Nx = Ni;

unsigned[4] Nj : dump;
alias numberOfPointsAlongAMeridian=Nj;
alias Ny = Nj;

alias geography.Ni=Ni;
alias geography.Nj=Nj;

#  Basic angle of the initial production domain
unsigned[4] basicAngleOfTheInitialProductionDomain = 0;
transient mBasicAngle=basicAngleOfTheInitialProductionDomain*oneMillionConstant;
transient angleMultiplier  = 1;
transient mAngleMultiplier = 1000000;
when (basicAngleOfTheInitialProductionDomain == 0) {
  set angleMultiplier  = 1;
  set mAngleMultiplier = 1000000;
} else {
  set angleMultiplier  = basicAngleOfTheInitialProductionDomain;
  set mAngleMultiplier = mBasicAngle;
}

#  Subdivisions of basic angle used to define extreme longitudes and latitudes, and direction increments
unsigned[4] subdivisionsOfBasicAngle = missing() : can_be_missing;

transient angleDivisor = 1000000;
when (missing(subdivisionsOfBasicAngle) || subdivisionsOfBasicAngle == 0) {
  set angleDivisor  = 1000000;
} else {
  set angleDivisor  = subdivisionsOfBasicAngle;
}

#  La1 - latitude of first grid point
signed[4] latitudeOfFirstGridPoint : edition_specific ;
alias La1  = latitudeOfFirstGridPoint;
#meta latitudeOfFirstGridPointInMicrodegrees times(latitudeOfFirstGridPoint,mAngleMultiplier,angleDivisor) : no_copy;

#  Lo1 - longitude of first grid point

signed[4] longitudeOfFirstGridPoint ;
alias Lo1  = longitudeOfFirstGridPoint;
#meta longitudeOfFirstGridPointInMicrodegrees times(longitudeOfFirstGridPoint,mAngleMultiplier,angleDivisor) : no_copy;

include "grib2/template.3.resolution_flags.def"

#  La2 - latitude of last grid point
signed[4] latitudeOfLastGridPoint :  edition_specific;
alias La2 =  latitudeOfLastGridPoint;
#meta latitudeOfLastGridPointInMicrodegrees times(latitudeOfLastGridPoint,mAngleMultiplier,angleDivisor) : no_copy;

#  Lo2 - longitude of last grid point
signed[4] longitudeOfLastGridPoint :  edition_specific ;
alias Lo2 =  longitudeOfLastGridPoint;
#meta longitudeOfLastGridPointInMicrodegrees times(longitudeOfLastGridPoint,mAngleMultiplier,angleDivisor) : no_copy;
